16 Jul 2019, 11:54:57
BARON

- ☐ fix engine brace that was removed when starter motor was replaced.
- ☐ make handbrake work
- ☐ Pipes on carb on top
- ☐ R5 mk1 dizzy right angle to make more space.
- ☐ 150 main jet too rich 130 too lean - 140 ok?
- ☐ 1st - 2nd stage - boost jet.
- ☐ Mega jolt ignition.
- ☐ Drill front bumper for intercooler
- ☐ Channel air for radiator
- ☐ Get oil cooler & fit, look at best place to put it, redirect air intake.
- ☐ Fix bumper back on properly
- ☐ Fit vent in bonnet
- ☐ Sort rust round windshield
- ☐ Switch wheels round
- ☐ Look for better seats?
- ☐ Put costs on spreadsheet
- ☐ 18mm X 1.5mm thread - metric with rose to make a compression fit. + 2m of oil pipe, reinforced so it doesn't kink. Note:Steel pipe OD = 12mm
- ☐
- ☑ weld hole in floor
- ☑ charge circuit needs fixing
- ☑ Starter motor earth frayed?
- ☑ fix switches in
- ☑ Refurbish front brakes callipers
- ☑ fit strut brace
- ☑ build and replace fuel pipes